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WHS Confined Space Entry Permit



	Airport
	Location
	Date



Details
	Employee/Contractor Name
	

	Contractor Address
	

	Emergency Contact Name
	Phone

	Name of Authorised Competent Person issuing Permit:
	

	Number of Entry Personnel (named in Section 8):
	

	JSEA or Procedure (name and number):
	Attach a copy to this permit

	Description of the Confined Space:
	

	
	

	Description of Work (if hot work, also complete Hot Work Permit for Confined Spaces):

	

	Hot Work Permit required? (please circle)
	Yes
	No


*Note: Ensure a Hot Work Permit is obtained and attached to this permit. Continuous atmospheric monitoring and continuous forced air ventilation/fume extraction is mandatory during hot work.

Isolations
The items below have been isolated or made safe:
	
	
	
	

	Pipelines (water, steam, gas, etc.)
	
	Harmful Materials
	

	Mechanical or Electrical Drives
	
	Electrical Services
	

	Sludges, Deposits, Waste
	
	Radiation
	

	Warning Notices, Portable Signs, Locks or Tags (danger) installed to the means of isolation
	



Atmospheric test requirements (fill in details of test)
	Has the gas detector been calibrated in the last 6 months? (please circle)
	Yes
	No


DO NOT USE GAS DETECTOR IF IT HAS NOT BEEN CALIBRATED IN LAST SIX (6) MONTHS
	Oxygen
	Flammable gases
	Other gases

	%
	%LEL
	ppm (less than…….ppm)

	%
	%LEL
	ppm (less than…….ppm)

	Other airborne contaminants

	

	


*Note: If the confined space must be cleared of contaminants then use a suitable purging agent. If the gas mixture has less than 21% by volume of oxygen, respiratory equipment must be provided.

The atmosphere is safe for entry under the conditions ticked:
	with supplied air respiratory device (no combustible gas)
	

	without supplied air respiratory device
	

	with an air purifying (non air supplied) respiratory protection device
	




Use of Chemical Agents
No chemical agents other than those listed below may be taken into the confined space.
	1. 
	2. 

	3. 
	4. 



Controls to be implemented
	
	
	
	

	1. Supplied air respirators (cylinders filled) reference to safe work procedures
	
	9. Safety helmets
	

	2. Air purifying respiratory protection devices
	
	10. Appropriate warning signs and barriers have been placed correctly
	

	3. Safety harness and/or safety line or lifeline/rescue
	
	11. Smoking has been banned from the confined space site
	

	4. Eye protection eg. safety glasses
	
	12. Ignition sources have been removed from within 6 metres of the entry/exit point
	

	5. Hand protection eg. gloves
	
	13. Equipment for fire protection
	

	6. Foot protection eg. safety shoes or boots
	
	14. First aid equipment
	

	7. Protective clothing eg. overalls
	
	15. No chemical agents other than those listed below shall be permitted
	

	8. Hearing protection
	
	16. Other special precautions required
	



Standby and Rescue Personnel
Standby personnel are:
	1. 
	2. 

	
	

	Rescue & emergency procedures have been issued and understood?    
	

	Openings for entry and exit to permit rescue of any person who may enter the confined space, or provision of suitable alternative means of rescue?
	

	Procedures to prevent obstruction of the openings by fittings or equipment which could impede rescue?
	

	Stand by persons are trained and understand they must not enter confined space?
	



Entry Personnel
We understand the safety procedures required for entry and exit for working in a confined space and the safety protective equipment to be used and have a working knowledge of the equipment to be used.

	NAME
	DATE OF
ENTRY
	IN
(TIME)
	SIGN
	OUT
(TIME)
	SIGN

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	

	
	
	
	
	
	



Authorisation for Entry (by Authorised Competent Person)
The confined space described above is, in my opinion, safe for the work detailed in the Description of Work above to be carried out, provided that the precautions listed are adhered to.
NOTE: No work shall be carried out within a confined space, or on the outside surface of a confined space, if the work or any plant is likely to cause or create a risk to the health and safety of a person in the confined space, or, of fire or explosion.
	Name
	Signature
	Date
	Time



	Permit valid from                      
	and expires on

	       :          am/pm on date           /         /
	         :         am/pm on date           /         /



Cancellation of written authority
All persons and equipment have been withdrawn and all signatories have signed off:
	Name
	Signature
	Date
	Time
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